(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "BQ7791506PW" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at -12.7 31.4706 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Value" "BQ7791506PW" (id 1) (at -12.7 -33.02 0)
      (effects (font (size 1.27 1.27)) (justify left bottom))
    )
    (property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "Datasheet" "https://www.ti.com/lit/ds/symlink/bq77915.pdf?ts=1666811225641&ref_url=https%253A%252F%252Fwww.ti.com%252Fproduct%252FBQ77915" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MANUFACTURER" "Texas Instruments" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "STANDARD" "IPC 7351B" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "PARTREV" "H" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify left bottom) hide)
    )
    (symbol "BQ7791506PW_0_0"
      (rectangle (start -12.7 -30.48) (end 12.7 30.48)
        (stroke (width 0.254) (type default) (color 0 0 0 0))
        (fill (type background))
      )
      (pin power_in line (at -17.78 27.94 0) (length 5.08)
        (name "VDD" (effects (font (size 1.016 1.016))))
        (number "1" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -7.62 0) (length 5.08)
        (name "SRP" (effects (font (size 1.016 1.016))))
        (number "10" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -10.16 0) (length 5.08)
        (name "SRN" (effects (font (size 1.016 1.016))))
        (number "11" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 -15.24 180) (length 5.08)
        (name "DSG" (effects (font (size 1.016 1.016))))
        (number "12" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 -12.7 180) (length 5.08)
        (name "CHG" (effects (font (size 1.016 1.016))))
        (number "13" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 -27.94 180) (length 5.08)
        (name "LD" (effects (font (size 1.016 1.016))))
        (number "14" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 -22.86 180) (length 5.08)
        (name "LPWR" (effects (font (size 1.016 1.016))))
        (number "15" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 -7.62 180) (length 5.08)
        (name "CBI" (effects (font (size 1.016 1.016))))
        (number "16" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 17.78 180) (length 5.08)
        (name "OCDP" (effects (font (size 1.016 1.016))))
        (number "17" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 10.16 180) (length 5.08)
        (name "TS" (effects (font (size 1.016 1.016))))
        (number "18" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 12.7 180) (length 5.08)
        (name "VTB" (effects (font (size 1.016 1.016))))
        (number "19" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 22.86 180) (length 5.08)
        (name "AVDD" (effects (font (size 1.016 1.016))))
        (number "2" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 22.86 0) (length 5.08)
        (name "CCFG" (effects (font (size 1.016 1.016))))
        (number "20" (effects (font (size 1.016 1.016))))
      )
      (pin output line (at 17.78 -5.08 180) (length 5.08)
        (name "CBO" (effects (font (size 1.016 1.016))))
        (number "21" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 -20.32 180) (length 5.08)
        (name "PRES" (effects (font (size 1.016 1.016))))
        (number "22" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 0 180) (length 5.08)
        (name "CTRC" (effects (font (size 1.016 1.016))))
        (number "23" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at 17.78 2.54 180) (length 5.08)
        (name "CTRD" (effects (font (size 1.016 1.016))))
        (number "24" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 10.16 0) (length 5.08)
        (name "VC5" (effects (font (size 1.016 1.016))))
        (number "3" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 7.62 0) (length 5.08)
        (name "VC4" (effects (font (size 1.016 1.016))))
        (number "4" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 5.08 0) (length 5.08)
        (name "VC3" (effects (font (size 1.016 1.016))))
        (number "5" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 2.54 0) (length 5.08)
        (name "VC2" (effects (font (size 1.016 1.016))))
        (number "6" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 0 0) (length 5.08)
        (name "VC1" (effects (font (size 1.016 1.016))))
        (number "7" (effects (font (size 1.016 1.016))))
      )
      (pin input line (at -17.78 -2.54 0) (length 5.08)
        (name "VC0" (effects (font (size 1.016 1.016))))
        (number "8" (effects (font (size 1.016 1.016))))
      )
      (pin power_in line (at -17.78 -27.94 0) (length 5.08)
        (name "VSS" (effects (font (size 1.016 1.016))))
        (number "9" (effects (font (size 1.016 1.016))))
      )
    )
  )
)
